           =-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

                      Adaptec EZ-SCSI Lite 4.01a README

                    (c) Copyright Adaptec, Inc.  1995-1996

           =-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=


=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=
Welcome to Adaptec EZ-SCSI Lite 4.01a
=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=


This README file explains how to install Adaptec EZ-SCSI Lite 4.0.  The
installation process copies a larger README.TXT file onto your hard drive
which explains Adaptec EZ-SCSI in greater detail.  If your questions are not
answered in this file please refer to the README.TXT file on your hard drive
after installation.


=-=-=-=-=-=-=-=
GETTING STARTED
=-=-=-=-=-=-=-=

Windows 95, Windows NT, or Windows 3.1/3.11
===========================================

  If running any of the above,insert the "Adaptec EZ-SCSI Setup Disk"
  into your floppy drive and run SETUP.EXE.

  Follow the instructions.

  When the Adaptec EZ-SCSI installation is complete, please select the
  "EZ-SCSI README" option for additional information.


DOS
===

  If running DOS, insert the "Adaptec EZ-SCSI Setup Disk" into your
  floppy drive, change to your floppy's drive letter, and run
  DOSINST.BAT.  For example:

        C:\> A:
        A:\> DOSINST <Enter>

  Follow the instructions.

  When the Adaptec EZ-SCSI installation is complete, please select the
  "EZ-SCSI README" option for additional information.

  