Trident 4dwave NX/DX Installation Instructions / Rev A / 7/18/2002
=================================================
The following instructions are for Windows 95/98. 
Procedure will be similar in other operating systems.
Please read through the entire readme file before installing driver.
=================================================

======================
A)General Notes:
======================
1) Unzip the archive, which you have already done, into a folder/directory.
	- Remember the folder location.
2) Make sure the old version of the 4dwave driver is removed.
	- Start > Settings > Control Panel > System > Device Manager
	- Sound, video, and game controllers
	- Find "Trident 4dwave(NX/DX) PCI Audio
	- Click on "Remove"
	- OK / Close Window
	- Reboot computer
3) After computer reboots, Windows will detect new hardware and will prompt for drivers.
4) Windows may ask for the Trident 4dwave Install CD. This is refering to the drivers you downloaded.

======================
Driver Installation:
======================
1) After rebooting, Windows will detect 3 devices related to the 4dwave.
	- These devices will be listed as "Unknown Device"
	- But will be ID'd by Windows to be either:
		"PCI multimedia Device" also "Trident 4dwave PCI Audio"
		"Trident Legacy Audio
		"Trident Direct Input Driver"
2) For each device, Windows will ask the location of the driver.
3) Either click "Browse" or manually type in the location of the downloaded driver.
	- i.e. "c:\4dwave"

======================
Specific Notes for:
======================
1) "PCI Multimedia Device" or "Trident 4dwave PCI Audio"
	- This device looks for the following file: "triaudio.inf"
2) "Trident Direct Input Driver"
	- This device looks for the following file: "tridinpt.inf"


